**Components that need attention**

|  |  |
| --- | --- |
| Footprint | CAP\_MP\_1608X90 |
| Reference | C16, C39, C72, C78  C28, C29, C49, C50, C94, C95, C186, C187 |
| Silk screen draw |  |
| 3D |  |
| Assemply drawing |  |
| Note | In silkscreen, the plus mark (+) is positive of the capacitor.  Dot in Assemply drawing: Anode (+) |